Raw data to reproduce Fig. 4

column 1: X component in CGS-EMU (multiply by 1000 to get A/m)
column 2: Y component in CGS-EMU (multiply by 1000 to get A/m)
column 3: Z component in CGS-EMU (multiply by 1000 to get A/m)
column 4: pTRM in CGS-EMU (multiply by 1000 to get A/m)
column 5: NRM in CGS-EMU (multiply by 1000 to get A/m)
column 6: normalized pTRM (by NRM0)
column 7: normalized NRM (by NRM0)
column 8: temperature in °C
column 9: pTRM check in CGS-EMU
column 10: normalized pTRM check (by NRM0)
column 11: error
column 12: temperature of the pTRM check in °C
column 13: pTRM tail check in CGS-EMU
column 14: normalized pTRM tail check (by NRM0)